


BIOS and Firmware Upgrade Steps :

* Before upgarde verify the verison.






* To proceed with upgrade, download the packages from the vendor site and import.




* Post import, reboot the server by choosing .






* After reboot, Legacy BIOS One-Time Boot menu will appear.




* Press Enter to enter the Legacy BIOS One-Time Boot.




* After Enter to Legacy BIOS One-Time Boot, it will take you to the below options.




* Choose the First option (One Time Boot to CD-ROM).




* Then you can get below two options (Automatic & Interative Firmware Update Version).





* Select Automatic Firmware Update Version (Suggested) and load with the imported package.





Continue… (Steps take care Automatically. No interation required)


































* Afetr completeion server automatically goes with reboot.




* Once boot up, login into the console.







* Verify the system ROM version and date (03/25/2019) which is latest before version.




* Then proceed with Firmware latest version upgrade. Choose Firmware tab.



* Select the Browse button to import the latest Firmware package.




* Download the package from the vendor site (P89\_2.74\_07\_21\_2019.signed.flash).




* During this ILO Firmware upgrade server reboot not required but it will case the ILO to reboot.

It will terminate any connections to ILO including Remote console and Virtual Media.


Make sure and Press OK to proceed.




* Then the uploading Firmware images will take place.




* Flashing Firmware image.





* Post compeltion proceed with reboot (suggested).







* Server is booting up.









* Login into the console and verify the ILO Firmware version.

